Run number

0 50 100 150 200 250 300 350

DMB input efficiency

0

0.2

0.4

0.6

0.8

1

ALCT DMB0 CLCT DMB0 CFEB DMB0

ALCT DMB1 CLCT DMB1 CFEB DMB1

ALCT DMB2 CLCT DMB2 CFEB DMB2

ALCT DMB3 CLCT DMB3 CFEB DMB3

ALCT DMB4 CLCT DMB4 CFEB DMB4